|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Test Writer: Jeremiah Franke | | | | | | | | | | | | |
| Test Case Name: | | | | | SPA User Test | | | | | Test ID#: | | USR-1 |
| Description: | | | | | A user test for functionality of the completed suspicious package training device. | | | | | Type: | | Black Box  White Box |
| Tester Information: | | | | | | | | | | | | |
| Name of Tester: | | |  | | | | | Date: | | |  | |
| Hardware Ver: | | | 1.0 | | | | | Time: | | |  | |
| Setup: | | | | | | | | Have device located in training environment. Have 9v battery and Oregon Zoo handheld radio. | | | | |
| Step | Action | Expected Result | | Pass | | Fail | N/A | | Comments | | | |
| 1 | Open battery compartment and install 9v battery. Close compartment. | Power LED off.  Active LED off. | |  | |  |  | |  | | | |
| 2 | Press power button to turn on device. | Power LED on.  Active LED off. | |  | |  |  | |  | | | |
| 3 | Wait for 30 seconds for activation. | Power LED on.  Active LED on. | |  | |  |  | |  | | | |
| 4 | Move training device. | Buzzer activated.  Failure LED is on. | |  | |  |  | |  | | | |
| 5 | Press reset switch. | Power LED on.  Buzzer off.  Failure LED off.  Active LED on. | |  | |  |  | |  | | | |
| 6 | Press talk button on Oregon Zoo radio. | Buzzer activated.  Failure LED is on. | |  | |  |  | |  | | | |
| 7 | Press power button to turn off device. | Power LED off.  Active LED off.  Buzzer off.  Failure LED off. | |  | |  |  | |  | | | |
| Overall test results: | | | |  | |  |  | |  | | | |